"eFM7" "eFMNEW7" "eFM77" "eFM77L2" - Fujitsu FM-7/FM-NEW7/FM-77/FM-77L2
								1/12/2018

--- Internal ROM image

    Main SYSTEM:
	BOOT_BAS.ROM    $FE00 - $FFFF BOOT ROM(Basic Mode)
	BOOT_DOS.ROM    $FE00 - $FFFF BOOT ROM(Dos Mode)
	BOOT_MMR.ROM    $FE00 - $FFFF BOOT ROM(MMR Mode / optional)
	
	Please select one of three:
	FBASIC.ROM	$8000 - $FBFF F-BASIC V3.0
	FBASIC300.ROM	$8000 - $FBFF F-BASIC V3.0
	FBASIC302.ROM	$8000 - $FBFF F-BASIC V3.0 L20

    Sub System:
	SUBSYS_C.ROM    $D800 - $FFFF Subsystem monitor and font.

    Optional:
	Please select one of two:
	KANJI1.ROM      JIS class 1 Kanji ROM $20000 bytes
	KANJI.ROM       JIS class 1 Kanji ROM $20000 bytes

	JSUBMON.ROM	Firmware of Japanese communication board (FM-7/77/AV). $4000 bytes.
	DICROM.ROM	Dictionary of Japanese communication board (FM-7/77/AV). $40000 bytes.
	                Same as external dictionary card for FM77AV40/EX/SX.
        JSUBKANJI.ROM	Kanji data of Japanese communication board (FM-7/77/AV). $20000 bytes.
	                If you don't have, KANJI.ROM/KANJI1.ROM is used for fallback.

--- Key maps

	Virtual		PC
	--------------------------------
	ESC		Kanji or Pause/Break
	BREAK		Esc
	Space		Muhenkan, Space and Henkan
	GRPH		Left ALT(Windows) or Left Windows key
	KANA		Katakana Hiragana
	INS		Insert
	DEL		Delete
	BS(⇐)		Back Space
	HOME		Home
	CLS		Page Down
	DUP		End
	EL		Page Up
	= (NUMPAD)	=	Scroll Lock(Windows) or Right Windows key
	Comma (NUMPAD)	Right Alt

	Anothe Keys include NUMPAD are refer to physical keyboard.
	
----------------------------------------
K.Ohta
whatisthis.sowhat@gmail.com
https://github.com/Artanejp/
Twitter @Artanejp

