The following is a list of files and features that are going to be
removed in the kernel source tree.  Every entry should contain what
exactly is going away, why it is happening, and who is going to be doing
the work.  When the feature is removed from the kernel, it should also
be removed from this file.

---------------------------

What:	x86 floppy disable_hlt
When:	2012
Why:	ancient workaround of dubious utility clutters the
	code used by everybody else.
Who:	Len Brown <len.brown@intel.com>

---------------------------

What:	CONFIG_APM_CPU_IDLE, and its ability to call APM BIOS in idle
When:	2012
Why:	This optional sub-feature of APM is of dubious reliability,
	and ancient APM laptops are likely better served by calling HLT.
	Deleting CONFIG_APM_CPU_IDLE allows x86 to stop exporting
	the pm_idle function pointer to modules.
Who:	Len Brown <len.brown@intel.com>

----------------------------

What:	x86_32 "no-hlt" cmdline param
When:	2012
Why:	remove a branch from idle path, simplify code used by everybody.
	This option disabled the use of HLT in idle and machine_halt()
	for hardware that was flakey 15-years ago.  Today we have
	"idle=poll" that removed HLT from idle, and so if such a machine
	is still running the upstream kernel, "idle=poll" is likely sufficient.
Who:	Len Brown <len.brown@intel.com>

----------------------------

What:	x86 "idle=mwait" cmdline param
When:	2012
Why:	simplify x86 idle code
Who:	Len Brown <len.brown@intel.com>

----------------------------

What:	PRISM54
When:	2.6.34

Why:	prism54 FullMAC PCI / Cardbus devices used to be supported only by the
	prism54 wireless driver. After Intersil stopped selling these
	devices in preference for the newer more flexible SoftMAC devices
	a SoftMAC device driver was required and prism54 did not support
	them. The p54pci driver now exists and has been present in the kernel for
	a while. This driver supports both SoftMAC devices and FullMAC devices.
	The main difference between these devices was the amount of memory which
	could be used for the firmware. The SoftMAC devices support a smaller
	amount of memory. Because of this the SoftMAC firmware fits into FullMAC
	devices's memory. p54pci supports not only PCI / Cardbus but also USB
	and SPI. Since p54pci supports all devices prism54 supports
	you will have a conflict. I'm not quite sure how distributions are
	handling this conflict right now. prism54 was kept around due to
	claims users may experience issues when using the SoftMAC driver.
	Time has passed users have not reported issues. If you use prism54
	and for whatever reason you cannot use p54pci please let us know!
	E-mail us at: linux-wireless@vger.kernel.org

	For more information see the p54 wiki page:

	http://wireless.kernel.org/en/users/Drivers/p54

Who:	Luis R. Rodriguez <lrodriguez@atheros.com>

---------------------------

What:	IRQF_SAMPLE_RANDOM
Check:	IRQF_SAMPLE_RANDOM
When:	July 2009

Why:	Many of IRQF_SAMPLE_RANDOM users are technically bogus as entropy
	sources in the kernel's current entropy model. To resolve this, every
	input point to the kernel's entropy pool needs to better document the
	type of entropy source it actually is. This will be replaced with
	additional add_*_randomness functions in drivers/char/random.c

Who:	Robin Getz <rgetz@blackfin.uclinux.org> & Matt Mackall <mpm@selenic.com>

---------------------------

What:	Deprecated snapshot ioctls
When:	2.6.36

Why:	The ioctls in kernel/power/user.c were marked as deprecated long time
	ago. Now they notify users about that so that they need to replace
	their userspace. After some more time, remove them completely.

Who:	Jiri Slaby <jirislaby@gmail.com>

---------------------------

What:	The ieee80211_regdom module parameter
When:	March 2010 / desktop catchup

Why:	This was inherited by the CONFIG_WIRELESS_OLD_REGULATORY code,
	and currently serves as an option for users to define an
	ISO / IEC 3166 alpha2 code for the country they are currently
	present in. Although there are userspace API replacements for this
	through nl80211 distributions haven't yet caught up with implementing
	decent alternatives through standard GUIs. Although available as an
	option through iw or wpa_supplicant its just a matter of time before
	distributions pick up good GUI options for this. The ideal solution
	would actually consist of intelligent designs which would do this for
	the user automatically even when travelling through different countries.
	Until then we leave this module parameter as a compromise.

	When userspace improves with reasonable widely-available alternatives for
	this we will no longer need this module parameter. This entry hopes that
	by the super-futuristically looking date of "March 2010" we will have
	such replacements widely available.

Who:	Luis R. Rodriguez <lrodriguez@atheros.com>

---------------------------

What:	dev->power.power_state
When:	July 2007
Why:	Broken design for runtime control over driver power states, confusing
	driver-internal runtime power management with:  mechanisms to support
	system-wide sleep state transitions; event codes that distinguish
	different phases of swsusp "sleep" transitions; and userspace policy
	inputs.  This framework was never widely used, and most attempts to
	use it were broken.  Drivers should instead be exposing domain-specific
	interfaces either to kernel or to userspace.
Who:	Pavel Machek <pavel@ucw.cz>

---------------------------

What:	sys_sysctl
When:	September 2010
Option: CONFIG_SYSCTL_SYSCALL
Why:	The same information is available in a more convenient from
	/proc/sys, and none of the sysctl variables appear to be
	important performance wise.

	Binary sysctls are a long standing source of subtle kernel
	bugs and security issues.

	When I looked several months ago all I could find after
	searching several distributions were 5 user space programs and
	glibc (which falls back to /proc/sys) using this syscall.

	The man page for sysctl(2) documents it as unusable for user
	space programs.

	sysctl(2) is not generally ABI compatible to a 32bit user
	space application on a 64bit and a 32bit kernel.

	For the last several months the policy has been no new binary
	sysctls and no one has put forward an argument to use them.

	Binary sysctls issues seem to keep happening appearing so
	properly deprecating them (with a warning to user space) and a
	2 year grace warning period will mean eventually we can kill
	them and end the pain.

	In the mean time individual binary sysctls can be dealt with
	in a piecewise fashion.

Who:	Eric Biederman <ebiederm@xmission.com>

---------------------------

What:	/proc/<pid>/oom_adj
When:	August 2012
Why:	/proc/<pid>/oom_adj allows userspace to influence the oom killer's
	badness heuristic used to determine which task to kill when the kernel
	is out of memory.

	The badness heuristic has since been rewritten since the introduction of
	this tunable such that its meaning is deprecated.  The value was
	implemented as a bitshift on a score generated by the badness()
	function that did not have any precise units of measure.  With the
	rewrite, the score is given as a proportion of available memory to the
	task allocating pages, so using a bitshift which grows the score
	exponentially is, thus, impossible to tune with fine granularity.

	A much more powerful interface, /proc/<pid>/oom_score_adj, was
	introduced with the oom killer rewrite that allows users to increase or
	decrease the badness score linearly.  This interface will replace
	/proc/<pid>/oom_adj.

	A warning will be emitted to the kernel log if an application uses this
	deprecated interface.  After it is printed once, future warnings will be
	suppressed until the kernel is rebooted.

---------------------------

What:	remove EXPORT_SYMBOL(kernel_thread)
When:	August 2006
Files:	arch/*/kernel/*_ksyms.c
Check:	kernel_thread
Why:	kernel_thread is a low-level implementation detail.  Drivers should
        use the <linux/kthread.h> API instead which shields them from
	implementation details and provides a higherlevel interface that
	prevents bugs and code duplication
Who:	Christoph Hellwig <hch@lst.de>

---------------------------

What:	Unused EXPORT_SYMBOL/EXPORT_SYMBOL_GPL exports
	(temporary transition config option provided until then)
	The transition config option will also be removed at the same time.
When:	before 2.6.19
Why:	Unused symbols are both increasing the size of the kernel binary
	and are often a sign of "wrong API"
Who:	Arjan van de Ven <arjan@linux.intel.com>

---------------------------

What:	PHYSDEVPATH, PHYSDEVBUS, PHYSDEVDRIVER in the uevent environment
When:	October 2008
Why:	The stacking of class devices makes these values misleading and
	inconsistent.
	Class devices should not carry any of these properties, and bus
	devices have SUBSYTEM and DRIVER as a replacement.
Who:	Kay Sievers <kay.sievers@suse.de>

---------------------------

What:	ACPI procfs interface
When:	July 2008
Why:	ACPI sysfs conversion should be finished by January 2008.
	ACPI procfs interface will be removed in July 2008 so that
	there is enough time for the user space to catch up.
Who:	Zhang Rui <rui.zhang@intel.com>

---------------------------

What:	CONFIG_ACPI_PROCFS_POWER
When:	2.6.39
Why:	sysfs I/F for ACPI power devices, including AC and Battery,
        has been working in upstream kernel since 2.6.24, Sep 2007.
	In 2.6.37, we make the sysfs I/F always built in and this option
	disabled by default.
	Remove this option and the ACPI power procfs interface in 2.6.39.
Who:	Zhang Rui <rui.zhang@intel.com>

---------------------------

What:	/proc/acpi/event
When:	February 2008
Why:	/proc/acpi/event has been replaced by events via the input layer
	and netlink since 2.6.23.
Who:	Len Brown <len.brown@intel.com>

---------------------------

What:	i386/x86_64 bzImage symlinks
When:	April 2010

Why:	The i386/x86_64 merge provides a symlink to the old bzImage
	location so not yet updated user space tools, e.g. package
	scripts, do not break.
Who:	Thomas Gleixner <tglx@linutronix.de>

---------------------------

What:	GPIO autorequest on gpio_direction_{input,output}() in gpiolib
When:	February 2010
Why:	All callers should use explicit gpio_request()/gpio_free().
	The autorequest mechanism in gpiolib was provided mostly as a
	migration aid for legacy GPIO interfaces (for SOC based GPIOs).
	Those users have now largely migrated.  Platforms implementing
	the GPIO interfaces without using gpiolib will see no changes.
Who:	David Brownell <dbrownell@users.sourceforge.net>
---------------------------

What:	b43 support for firmware revision < 410
When:	The schedule was July 2008, but it was decided that we are going to keep the
        code as long as there are no major maintanance headaches.
	So it _could_ be removed _any_ time now, if it conflicts with something new.
Why:	The support code for the old firmware hurts code readability/maintainability
	and slightly hurts runtime performance. Bugfixes for the old firmware
	are not provided by Broadcom anymore.
Who:	Michael Buesch <m@bues.ch>

---------------------------

What:	Ability for non root users to shm_get hugetlb pages based on mlock
	resource limits
When:	2.6.31
Why:	Non root users need to be part of /proc/sys/vm/hugetlb_shm_group or
	have CAP_IPC_LOCK to be able to allocate shm segments backed by
	huge pages.  The mlock based rlimit check to allow shm hugetlb is
	inconsistent with mmap based allocations.  Hence it is being
	deprecated.
Who:	Ravikiran Thirumalai <kiran@scalex86.org>

---------------------------

What:	Code that is now under CONFIG_WIRELESS_EXT_SYSFS
	(in net/core/net-sysfs.c)
When:	After the only user (hal) has seen a release with the patches
	for enough time, probably some time in 2010.
Why:	Over 1K .text/.data size reduction, data is available in other
	ways (ioctls)
Who:	Johannes Berg <johannes@sipsolutions.net>

---------------------------

What:	sysfs ui for changing p4-clockmod parameters
When:	September 2009
Why:	See commits 129f8ae9b1b5be94517da76009ea956e89104ce8 and
	e088e4c9cdb618675874becb91b2fd581ee707e6.
	Removal is subject to fixing any remaining bugs in ACPI which may
	cause the thermal throttling not to happen at the right time.
Who:	Dave Jones <davej@redhat.com>, Matthew Garrett <mjg@redhat.com>

-----------------------------

What:	fakephp and associated sysfs files in /sys/bus/pci/slots/
When:	2011
Why:	In 2.6.27, the semantics of /sys/bus/pci/slots was redefined to
	represent a machine's physical PCI slots. The change in semantics
	had userspace implications, as the hotplug core no longer allowed
	drivers to create multiple sysfs files per physical slot (required
	for multi-function devices, e.g.). fakephp was seen as a developer's
	tool only, and its interface changed. Too late, we learned that
	there were some users of the fakephp interface.

	In 2.6.30, the original fakephp interface was restored. At the same
	time, the PCI core gained the ability that fakephp provided, namely
	function-level hot-remove and hot-add.

	Since the PCI core now provides the same functionality, exposed in:

		/sys/bus/pci/rescan
		/sys/bus/pci/devices/.../remove
		/sys/bus/pci/devices/.../rescan

	there is no functional reason to maintain fakephp as well.

	We will keep the existing module so that 'modprobe fakephp' will
	present the old /sys/bus/pci/slots/... interface for compatibility,
	but users are urged to migrate their applications to the API above.

	After a reasonable transition period, we will remove the legacy
	fakephp interface.
Who:	Alex Chiang <achiang@hp.com>

---------------------------

What:	CONFIG_RFKILL_INPUT
When:	2.6.33
Why:	Should be implemented in userspace, policy daemon.
Who:	Johannes Berg <johannes@sipsolutions.net>

----------------------------

What:	sound-slot/service-* module aliases and related clutters in
	sound/sound_core.c
When:	August 2010
Why:	OSS sound_core grabs all legacy minors (0-255) of SOUND_MAJOR
	(14) and requests modules using custom sound-slot/service-*
	module aliases.  The only benefit of doing this is allowing
	use of custom module aliases which might as well be considered
	a bug at this point.  This preemptive claiming prevents
	alternative OSS implementations.

	Till the feature is removed, the kernel will be requesting
	both sound-slot/service-* and the standard char-major-* module
	aliases and allow turning off the pre-claiming selectively via
	CONFIG_SOUND_OSS_CORE_PRECLAIM and soundcore.preclaim_oss
	kernel parameter.

	After the transition phase is complete, both the custom module
	aliases and switches to disable it will go away.  This removal
	will also allow making ALSA OSS emulation independent of
	sound_core.  The dependency will be broken then too.
Who:	Tejun Heo <tj@kernel.org>

----------------------------

What:	sysfs-class-rfkill state file
When:	Feb 2014
Files:	net/rfkill/core.c
Why: 	Documented as obsolete since Feb 2010. This file is limited to 3
	states while the rfkill drivers can have 4 states.
Who: 	anybody or Florian Mickler <florian@mickler.org>

----------------------------

What: 	sysfs-class-rfkill claim file
When:	Feb 2012
Files:	net/rfkill/core.c
Why:	It is not possible to claim an rfkill driver since 2007. This is
	Documented as obsolete since Feb 2010.
Who: 	anybody or Florian Mickler <florian@mickler.org>

----------------------------

What:	KVM paravirt mmu host support
When:	January 2011
Why:	The paravirt mmu host support is slower than non-paravirt mmu, both
	on newer and older hardware.  It is already not exposed to the guest,
	and kept only for live migration purposes.
Who:	Avi Kivity <avi@redhat.com>

----------------------------

What:	iwlwifi 50XX module parameters
When:	3.0
Why:	The "..50" modules parameters were used to configure 5000 series and
	up devices; different set of module parameters also available for 4965
	with same functionalities. Consolidate both set into single place
	in drivers/net/wireless/iwlwifi/iwl-agn.c

Who:	Wey-Yi Guy <wey-yi.w.guy@intel.com>

----------------------------

What:	iwl4965 alias support
When:	3.0
Why:	Internal alias support has been present in module-init-tools for some
	time, the MODULE_ALIAS("iwl4965") boilerplate aliases can be removed
	with no impact.

Who:	Wey-Yi Guy <wey-yi.w.guy@intel.com>

---------------------------

What:	xt_NOTRACK
Files:	net/netfilter/xt_NOTRACK.c
When:	April 2011
Why:	Superseded by xt_CT
Who:	Netfilter developer team <netfilter-devel@vger.kernel.org>

----------------------------

What:	IRQF_DISABLED
When:	2.6.36
Why:	The flag is a NOOP as we run interrupt handlers with interrupts disabled
Who:	Thomas Gleixner <tglx@linutronix.de>

----------------------------

What: 	PCI DMA unmap state API
When:	August 2012
Why:	PCI DMA unmap state API (include/linux/pci-dma.h) was replaced
	with DMA unmap state API (DMA unmap state API can be used for
	any bus).
Who:	FUJITA Tomonori <fujita.tomonori@lab.ntt.co.jp>

----------------------------

What:	iwlwifi disable_hw_scan module parameters
When:	3.0
Why:	Hareware scan is the prefer method for iwlwifi devices for
	scanning operation. Remove software scan support for all the
	iwlwifi devices.

Who:	Wey-Yi Guy <wey-yi.w.guy@intel.com>

----------------------------

What:	Legacy, non-standard chassis intrusion detection interface.
When:	June 2011
Why:	The adm9240, w83792d and w83793 hardware monitoring drivers have
	legacy interfaces for chassis intrusion detection. A standard
	interface has been added to each driver, so the legacy interface
	can be removed.
Who:	Jean Delvare <khali@linux-fr.org>

----------------------------

What:	xt_connlimit rev 0
When:	2012
Who:	Jan Engelhardt <jengelh@medozas.de>
Files:	net/netfilter/xt_connlimit.c

----------------------------

What:	ipt_addrtype match include file
When:	2012
Why:	superseded by xt_addrtype
Who:	Florian Westphal <fw@strlen.de>
Files:	include/linux/netfilter_ipv4/ipt_addrtype.h

----------------------------

What:	i2c_driver.attach_adapter
	i2c_driver.detach_adapter
When:	September 2011
Why:	These legacy callbacks should no longer be used as i2c-core offers
	a variety of preferable alternative ways to instantiate I2C devices.
Who:	Jean Delvare <khali@linux-fr.org>

----------------------------

What:	Support for UVCIOC_CTRL_ADD in the uvcvideo driver
When:	3.2
Why:	The information passed to the driver by this ioctl is now queried
	dynamically from the device.
Who:	Laurent Pinchart <laurent.pinchart@ideasonboard.com>

----------------------------

What:	Support for UVCIOC_CTRL_MAP_OLD in the uvcvideo driver
When:	3.2
Why:	Used only by applications compiled against older driver versions.
	Superseded by UVCIOC_CTRL_MAP which supports V4L2 menu controls.
Who:	Laurent Pinchart <laurent.pinchart@ideasonboard.com>

----------------------------

What:	Support for UVCIOC_CTRL_GET and UVCIOC_CTRL_SET in the uvcvideo driver
When:	3.2
Why:	Superseded by the UVCIOC_CTRL_QUERY ioctl.
Who:	Laurent Pinchart <laurent.pinchart@ideasonboard.com>

----------------------------

What:	Support for driver specific ioctls in the pwc driver (everything
	defined in media/pwc-ioctl.h)
When:	3.3
Why:	This stems from the v4l1 era, with v4l2 everything can be done with
	standardized v4l2 API calls
Who:	Hans de Goede <hdegoede@redhat.com>

----------------------------

What:	Driver specific sysfs API in the pwc driver
When:	3.3
Why:	Setting pan/tilt should be done with v4l2 controls, like with other
	cams. The button is available as a standard input device
Who:	Hans de Goede <hdegoede@redhat.com>

----------------------------

What:	Driver specific use of pixfmt.priv in the pwc driver
When:	3.3
Why:	The .priv field never was intended for this, setting a framerate is
	support using the standardized S_PARM ioctl
Who:	Hans de Goede <hdegoede@redhat.com>

----------------------------

What:	Software emulation of arbritary resolutions in the pwc driver
When:	3.3
Why:	The pwc driver claims to support any resolution between 160x120
	and 640x480, but emulates this by simply drawing a black border
	around the image. Userspace can draw its own black border if it
	really wants one.
Who:	Hans de Goede <hdegoede@redhat.com>

----------------------------

What:	For VIDIOC_S_FREQUENCY the type field must match the device node's type.
	If not, return -EINVAL.
When:	3.2
Why:	It makes no sense to switch the tuner to radio mode by calling
	VIDIOC_S_FREQUENCY on a video node, or to switch the tuner to tv mode by
	calling VIDIOC_S_FREQUENCY on a radio node. This is the first step of a
	move to more consistent handling of tv and radio tuners.
Who:	Hans Verkuil <hans.verkuil@cisco.com>

----------------------------

What:	Opening a radio device node will no longer automatically switch the
	tuner mode from tv to radio.
When:	3.3
Why:	Just opening a V4L device should not change the state of the hardware
	like that. It's very unexpected and against the V4L spec. Instead, you
	switch to radio mode by calling VIDIOC_S_FREQUENCY. This is the second
	and last step of the move to consistent handling of tv and radio tuners.
Who:	Hans Verkuil <hans.verkuil@cisco.com>

----------------------------

What:	g_file_storage driver
When:	3.8
Why:	This driver has been superseded by g_mass_storage.
Who:	Alan Stern <stern@rowland.harvard.edu>

----------------------------

What:   threeg and interface sysfs files in /sys/devices/platform/acer-wmi
When:   2012
Why:    In 3.0, we can now autodetect internal 3G device and already have
	the threeg rfkill device. So, we plan to remove threeg sysfs support
	for it's no longer necessary.

	We also plan to remove interface sysfs file that exposed which ACPI-WMI
	interface that was used by acer-wmi driver. It will replaced by
	information log when acer-wmi initial.
Who:    Lee, Chun-Yi <jlee@novell.com>
