Wireshark 2.9.0-477-g68ec514b The Wireshark network protocol analyzer

- Main Page
- Related Pages
- Modules
- Namespaces
- Classes
- Files

- File List
- File Members

bridged_pids.h
1 /* bridged_pids.h
2 * Definitions of protocol IDs for the 00-80-C2 OUI, used for
3 * bridging various networks over ATM (RFC 2684) or Frame Relay (RFC 2427).
4 *
5 * Wireshark - Network traffic analyzer
6 * By Gerald Combs <gerald@wireshark.org>
7 * Copyright 1998 - 2000 Gerald Combs
8 *
9 * SPDX-License-Identifier: GPL-2.0-or-later
10 */
11
12 #ifndef __BRIDGED_PID_H__
13 #define __BRIDGED_PID_H__
14
15 #ifdef __cplusplus
16 extern "C" {
17 #endif /* __cplusplus */
18
19 #define BPID_ETH_WITH_FCS 0x0001 /* 802.3/Ethernet with preserved FCS */
20 #define BPID_ETH_WITHOUT_FCS 0x0007 /* 802.3/Ethernet without preserved FCS */
21
22 #define BPID_802_4_WITH_FCS 0x0002 /* 802.4 with preserved FCS */
23 #define BPID_802_4_WITHOUT_FCS 0x0008 /* 802.4 without preserved FCS */
24
25 #define BPID_802_5_WITH_FCS 0x0003 /* 802.5 with preserved FCS */
26 #define BPID_802_5_WITHOUT_FCS 0x0009 /* 802.5 without preserved FCS */
27
28 #define BPID_FDDI_WITH_FCS 0x0004 /* FDDI with preserved FCS */
29 #define BPID_FDDI_WITHOUT_FCS 0x000A /* FDDI without preserved FCS */
30
31 #define BPID_802_6_WITH_FCS 0x0005 /* 802.6 with preserved FCS */
32 #define BPID_802_6_WITHOUT_FCS 0x000B /* 802.6 without preserved FCS */
33
34 #define BPID_FRAGMENTS 0x000D
35
36 #define BPID_BPDU 0x000E /* 802.1(d) or 802.1(g) BPDUs */
37
38 #define BPID_SR_BPDU 0x000F /* Source Routing BPDUs */
39
40 #ifdef __cplusplus
41 }
42 #endif /* __cplusplus */
43
44 #endif /* bridged_pid.h */