Wireshark 2.9.0-477-g68ec514b The Wireshark network protocol analyzer

- Main Page
- Related Pages
- Modules
- Namespaces
- Classes
- Files

- Class List
- Class Index
- Class Hierarchy
- Class Members

Public Attributes | List of all members
_seq_analysis_item Struct Reference

`#include <sequence_analysis.h>`

## Public Attributes
guint32 | frame_number
address | src_addr
guint16 | port_src
address | dst_addr
guint16 | port_dst
gchar * | frame_label
gchar * | time_str
gchar * | comment
guint16 | conv_num
unsigned | fg_color
unsigned | bg_color
gboolean | has_color_filter
gboolean | display
guint | src_node
guint | dst_node
guint16 | line_style

## Detailed Description

defines an entry for the graph analysis

## Member Data Documentation

unsigned _seq_analysis_item::bg_color

Background color, 0xRRGGBB. Qt only.

gchar* _seq_analysis_item::comment

a comment that appears at the right of the graph

guint16 _seq_analysis_item::conv_num

The conversation number. Used for coloring VoIP calls.

gboolean _seq_analysis_item::display

indicate if the packet is displayed or not in the graph

guint _seq_analysis_item::dst_node

a node is an IP address that will be displayed in columns

unsigned _seq_analysis_item::fg_color

Foreground color, 0xRRGGBB. Qt only.

gchar* _seq_analysis_item::frame_label

the label on top of the arrow

gboolean _seq_analysis_item::has_color_filter

Set if packet has color filter. Qt only.

guint16 _seq_analysis_item::line_style

the arrow line width in pixels

guint _seq_analysis_item::src_node

this is used by graph_analysis.c to identify the node

gchar* _seq_analysis_item::time_str

timestamp

The documentation for this struct was generated from the following file:

- /home/wireshark/builders/wireshark-master/ubuntu-16.04-x64/build/epan/sequence_analysis.h