Wireshark 2.9.0-477-g68ec514b The Wireshark network protocol analyzer

- Main Page
- Related Pages
- Modules
- Namespaces
- Classes
- Files

- File List
- File Members

ipproto.h
1 /* ipproto.h
2 * Declarations of IP protocol numbers, and of routines for converting
3 * IP protocol numbers into strings.
4 *
5 * Wireshark - Network traffic analyzer
6 * By Gerald Combs <gerald@wireshark.org>
7 * Copyright 1998 Gerald Combs
8 *
9 * SPDX-License-Identifier: GPL-2.0-or-later
10 */
11
12 #ifndef __IPPROTO_H__
13 #define __IPPROTO_H__
14
15 #include "ws_symbol_export.h"
16
17 /*
18 * IP protocol numbers.
19 * http://www.iana.org/assignments/protocol-numbers/protocol-numbers.xml
20 */
21 #define IP_PROTO_HOPOPTS 0 /* IP6 hop-by-hop options - RFC1883 */
22 #define IP_PROTO_ICMP 1 /* control message protocol - RFC792 */
23 #define IP_PROTO_IGMP 2 /* group mgmt protocol - RFC1112 */
24 #define IP_PROTO_GGP 3 /* gateway^2 (deprecated) - RFC823*/
25 #define IP_PROTO_IPIP 4 /* IP inside IP - RFC2003*/
26 #define IP_PROTO_IPV4 4 /* IP header */
27 #define IP_PROTO_STREAM 5 /* Stream - RFC1190, RFC1819 */
28 #define IP_PROTO_TCP 6 /* TCP - RFC792 */
29 #define IP_PROTO_CBT 7 /* CBT - <A.Ballardie@cs.ucl.ac.uk> */
30 #define IP_PROTO_EGP 8 /* exterior gateway protocol - RFC888 */
31 #define IP_PROTO_IGP 9 /* any private interior gateway protocol ... */
32 #define IP_PROTO_IGRP 9 /* ... and used by Cisco for IGRP */
33 #define IP_PROTO_BBN_RCC 10 /* BBN RCC Monitoring */
34 #define IP_PROTO_NVPII 11 /* Network Voice Protocol - RFC741 */
35 #define IP_PROTO_PUP 12 /* pup */
36 #define IP_PROTO_ARGUS 13 /* ARGUS */
37 #define IP_PROTO_EMCON 14 /* EMCON */
38 #define IP_PROTO_XNET 15 /* Cross net debugger - IEN158 */
39 #define IP_PROTO_CHAOS 16 /* CHAOS */
40 #define IP_PROTO_UDP 17 /* user datagram protocol - RFC768 */
41 #define IP_PROTO_MUX 18 /* multiplexing - IEN90 */
42 #define IP_PROTO_DCNMEAS 19 /* DCN Measurement Subsystems */
43 #define IP_PROTO_HMP 20 /* Host Monitoring - RFC869 */
44 #define IP_PROTO_PRM 21 /* Packet radio measurement */
45 #define IP_PROTO_IDP 22 /* xns idp */
46 #define IP_PROTO_TRUNK1 23
47 #define IP_PROTO_TRUNK2 24
48 #define IP_PROTO_LEAF1 25
49 #define IP_PROTO_LEAF2 26
50 #define IP_PROTO_RDP 27 /* Reliable Data Protocol - RFC908 */
51 #define IP_PROTO_IRT 28 /* Internet Reliable Transation - RFC938 */
52 #define IP_PROTO_TP 29 /* tp-4 w/ class negotiation - RFC905 */
53 #define IP_PROTO_BULK 30 /* Bulk Data Transfer Protocol - RFC969 */
54 #define IP_PROTO_MFE_NSP 31 /* MFE Network Services Protocol */
55 #define IP_PROTO_MERIT 32 /* MERIT Internodal Protocol */
56 #define IP_PROTO_DCCP 33 /* Datagram Congestion Control Protocol */
57 #define IP_PROTO_3PC 34 /* Third party connect protocol */
58 #define IP_PROTO_IDPR 35 /* Interdomain policy routing protocol */
59 #define IP_PROTO_XTP 36 /* Xpress Transport Protocol */
60 #define IP_PROTO_DDP 37 /* Datagram Delivery Protocol */
61 #define IP_PROTO_CMTP 38 /* Control Message Transport Protocol */
62 #define IP_PROTO_TPPP 39 /* TP++ Transport Protocol */
63 #define IP_PROTO_IL 40 /* IL Transport Protocol */
64 #define IP_PROTO_IPV6 41 /* IP6 header */
65 #define IP_PROTO_SDRP 42 /* Source demand routing protocol */
66 #define IP_PROTO_ROUTING 43 /* IP6 routing header */
67 #define IP_PROTO_FRAGMENT 44 /* IP6 fragmentation header */
68 #define IP_PROTO_IDRP 45 /* Inter-Domain Routing Protocol */
69 #define IP_PROTO_RSVP 46 /* Resource ReSerVation protocol */
70 #define IP_PROTO_GRE 47 /* General Routing Encapsulation */
71 #define IP_PROTO_DSR 48 /* Dynamic Source Routing Protocol */
72 #define IP_PROTO_BNA 49 /* BNA */
73 #define IP_PROTO_ESP 50 /* Encap Security Payload for IPv6 - RFC2406 */
74 #define IP_PROTO_AH 51 /* Authentication Header for IPv6 - RFC2402*/
75 #define IP_PROTO_INSLP 52 /* Integrated Net Layer Security */
76 #define IP_PROTO_SWIPE 53 /* IP with Encryption */
77 #define IP_PROTO_NARP 54 /* NBMA Address resolution protocol - RFC1735 */
78 #define IP_PROTO_MOBILE 55 /* IP Mobility */
79 #define IP_PROTO_TLSP 56 /* Transport Layer Security Protocol using */
80 /* Kryptonet key management */
81 #define IP_PROTO_SKIP 57 /* SKIP */
82 #define IP_PROTO_ICMPV6 58 /* ICMP6 - RFC1883*/
83 #define IP_PROTO_NONE 59 /* IP6 no next header - RFC1883 */
84 #define IP_PROTO_DSTOPTS 60 /* IP6 destination options - RFC1883 */
85 /* 61 is reserved by IANA for any host internal protocol */
86
87 /*
88 * The current Protocol Numbers list says that the IP protocol number for
89 * mobility headers is 135; it cites draft-ietf-mobileip-ipv6-24, but
90 * that draft doesn't actually give a number.
91 *
92 * It appears that 62 used to be used, even though that's assigned to
93 * a protocol called CFTP; however, the only reference for CFTP is a
94 * Network Message from BBN back in 1982, so, for now, we support 62,
95 * as well as 135, as a protocol number for mobility headers.
96 */
97 #define IP_PROTO_MIPV6_OLD 62 /* Mobile IPv6 */
98 /* 63 is reserved by IANA for any local network */
99 #define IP_PROTO_SATEXPAK 64
100 #define IP_PROTO_KRYPTOLAN 65
101 #define IP_PROTO_RVD 66 /* MIT Remote virtual disk protocol */
102 #define IP_PROTO_IPPC 67 /* Internet Pluribus Packet Core */
103 /* 68 is reserved by IANA for any distributed file system */
104 #define IP_PROTO_SATMON 69 /* SATNET Monitoring */
105 #define IP_PROTO_VISA 70 /* VISA Protocol */
106 #define IP_PROTO_IPCV 71 /* Internet Packet Core Utility */
107 #define IP_PROTO_CPNX 72 /* Computer Protocol Network Executive */
108 #define IP_PROTO_CPHB 73 /* Computer Protocol Heart Beat */
109 #define IP_PROTO_WSN 74 /* WANG Span Network */
110 #define IP_PROTO_PVP 75 /* Packet Video Protocol */
111 #define IP_PROTO_BRSATMON 76 /* Backroon SATNET Monitoring */
112 #define IP_PROTO_SUNND 77 /* SUN ND Protocol - Temporary */
113 #define IP_PROTO_WBMON 78 /* Wideband Monitoring */
114 #define IP_PROTO_WBEXPAK 79 /* Wideband EXPAK */
115 #define IP_PROTO_ISOIP 80 /* ISO IP */
116 #define IP_PROTO_VMTP 81
117 #define IP_PROTO_SVMTP 82 /* Secure VMTP */
118 #define IP_PROTO_VINES 83 /* Vines over raw IP */
119 #define IP_PROTO_TTP 84
120 #define IP_PROTO_NSFNETIGP 85 /* NSFNET IGP */
121 #define IP_PROTO_DGP 86 /* Dissimilar Gateway Protocol */
122 #define IP_PROTO_TCF 87
123 #define IP_PROTO_EIGRP 88
124 #define IP_PROTO_OSPF 89 /* OSPF Interior Gateway Protocol - RFC1583 */
125 #define IP_PROTO_SPRITE 90 /* SPRITE RPC protocol */
126 #define IP_PROTO_LARP 91 /* Locus Address Resolution Protocol */
127 #define IP_PROTO_MTP 92 /* Multicast Transport Protocol */
128 #define IP_PROTO_AX25 93 /* AX.25 frames */
129 #define IP_PROTO_IPINIP 94 /* IP within IP Encapsulation protocol */
130 #define IP_PROTO_MICP 95 /* Mobile Internetworking Control Protocol */
131 #define IP_PROTO_SCCCP 96 /* Semaphore communications security protocol */
132 #define IP_PROTO_ETHERIP 97 /* Ethernet-within-IP - RFC 3378 */
133 #define IP_PROTO_ENCAP 98 /* encapsulation header - RFC1241*/
134 /* 99 is reserved by IANA for any private encryption scheme */
135 #define IP_PROTO_GMTP 100
136 #define IP_PROTO_IFMP 101 /* Ipsilon flow management protocol */
137 #define IP_PROTO_PNNI 102 /* PNNI over IP */
138 #define IP_PROTO_PIM 103 /* Protocol Independent Mcast */
139 #define IP_PROTO_ARIS 104
140 #define IP_PROTO_SCPS 105
141 #define IP_PROTO_QNX 106
142 #define IP_PROTO_AN 107 /* Active Networks */
143 #define IP_PROTO_IPCOMP 108 /* IP payload compression - RFC2393 */
144 #define IP_PROTO_SNP 109 /* Sitara Networks Protocol */
145 #define IP_PROTO_COMPAQ 110 /* Compaq Peer Protocol */
146 #define IP_PROTO_IPX 111 /* IPX over IP */
147 #define IP_PROTO_VRRP 112 /* Virtual Router Redundancy Protocol */
148 #define IP_PROTO_PGM 113 /* Pragmatic General Multicast */
149 /* 114 is reserved by IANA for any zero hop protocol */
150 #define IP_PROTO_L2TP 115 /* Layer Two Tunnelling Protocol */
151 #define IP_PROTO_DDX 116 /* D-II Data Exchange */
152 #define IP_PROTO_IATP 117 /* Interactive Agent Transfer Protocol */
153 #define IP_PROTO_STP 118 /* Schedule Transfer Protocol */
154 #define IP_PROTO_SRP 119 /* Spectralink Radio Protocol */
155 #define IP_PROTO_UTI 120
156 #define IP_PROTO_SMP 121 /* Simple Message Protocol */
157 #define IP_PROTO_SM 122
158 #define IP_PROTO_PTP 123 /* Performance Transparency Protocol */
159 #define IP_PROTO_ISIS 124 /* ISIS over IPv4 */
160 #define IP_PROTO_FIRE 125
161 #define IP_PROTO_CRTP 126 /* Combat Radio Transport Protocol */
162 #define IP_PROTO_CRUDP 127 /* Combat Radio User Datagram */
163 #define IP_PROTO_SSCOPMCE 128
164 #define IP_PROTO_IPLT 129
165 #define IP_PROTO_SPS 130 /* Secure Packet Shield */
166 #define IP_PROTO_PIPE 131 /* Private IP Encapsulation within IP */
167 #define IP_PROTO_SCTP 132 /* Stream Control Transmission Protocol */
168 #define IP_PROTO_FC 133 /* Fibre Channel */
169 #define IP_PROTO_RSVPE2EI 134 /* RSVP E2E Ignore - RFC3175 */
170 #define IP_PROTO_MIPV6 135 /* Mobile IPv6 */
171 #define IP_PROTO_UDPLITE 136 /* Lightweight user datagram protocol - RFC3828 */
172 #define IP_PROTO_MPLS_IN_IP 137 /* MPLS in IP - RFC4023 */
173 #define IP_PROTO_MANET 138 /* MANET Protocols */
174 #define IP_PROTO_HIP 139 /* Host Identity Protocol */
175 #define IP_PROTO_SHIM6 140 /* Shim6 Protocol */
176 #define IP_PROTO_WESP 141 /* 141 WESP Wrapped Encapsulating Security Payload [RFC5840] */
177 #define IP_PROTO_ROHC 142 /* 142 ROHC Robust Header Compression [RFC5858] */
178 #define IP_PROTO_AX4000 173 /* AX/4000 Testblock - non IANA */
179 #define IP_PROTO_NCS_HEARTBEAT 224 /* Novell NCS Heartbeat - http://support.novell.com/cgi-bin/search/searchtid.cgi?/10071158.htm */
180
181 WS_DLL_PUBLIC value_string_ext ipproto_val_ext;
182 WS_DLL_PUBLIC const char *ipprotostr(const int proto);
183
184 WS_DLL_PUBLIC const char *ipv6extprotostr(int proto);
185
186 #endif /* ipproto.h */
187
188 /*
189 * Editor modelines
190 *
191 * Local Variables:
192 * c-basic-offset: 4
193 * tab-width: 8
194 * indent-tabs-mode: nil
195 * End:
196 *
197 * ex: set shiftwidth=4 tabstop=8 expandtab:
198 * :indentSize=4:tabSize=8:noTabs=true:
199 */
_value_string_ext
Definition: value_string.h:164