Wireshark 2.9.0-477-g68ec514b The Wireshark network protocol analyzer

- Main Page
- Related Pages
- Modules
- Namespaces
- Classes
- Files

- Class List
- Class Index
- Class Hierarchy
- Class Members

Public Attributes | List of all members
mac_lte_info Struct Reference

## Public Attributes
guint8 | radioType
guint8 | direction
guint8 | rntiType
guint16 | rnti
guint16 | ueid
guint16 | sysframeNumber
guint16 | subframeNumber
gboolean | subframeNumberOfGrantPresent
guint16 | subframeNumberOfGrant
gboolean | isPredefinedData
guint16 | length
guint8 | reTxCount
guint8 | isPHICHNACK
gboolean | isExtendedBSRSizes
gboolean | isSimultPUCCHPUSCHPCell
gboolean | isSimultPUCCHPUSCHPSCell
gboolean | crcStatusValid
mac_lte_crc_status | crcStatus
mac_lte_carrier_id | carrierId
mac_lte_dl_retx | dl_retx
mac_lte_ce_mode | ceMode
mac_lte_nb_mode | nbMode
guint8 | nUlRb
union {
struct mac_lte_ul_phy_info {
guint8 present
guint8 modulation_type
guint8 tbs_index
guint8 resource_block_length
guint8 resource_block_start
guint8 harq_id
gboolean ndi
} ul_info
struct mac_lte_dl_phy_info {
guint8 present
guint8 dci_format
guint8 resource_allocation_type
guint8 aggregation_level
guint8 mcs_index
guint8 redundancy_version_index
guint8 resource_block_length
guint8 harq_id
gboolean ndi
guint8 transport_block
} dl_info
} | detailed_phy_info
mac_lte_oob_event | oob_event
guint8 | rapid
guint8 | rach_attempt_number
guint16 | number_of_srs
guint16 | oob_ueid [MAX_SRs]
guint16 | oob_rnti [MAX_SRs]

The documentation for this struct was generated from the following file:

- /home/wireshark/builders/wireshark-master/ubuntu-16.04-x64/build/epan/dissectors/packet-mac-lte.h